**Kachemak Bay Research Reserve (KAC) NERR Water Quality Metadata**

**January – December 2013**

**Latest update:** 03/11/2014

Note: This is a provisional metadata document; it has not been authenticated as of its download date. Contents of this document are subject to change throughout the QAQC process and it should not be considered a final record of data documentation until that process is complete. Contact the CDMO ([cdmosupport@belle.baruch.sc.edu](mailto:cdmosupport@belle.baruch.sc.edu)) or Reserve with any additional questions.

**I. Data Set and Research Descriptors**

**1) Principal Investigators & Contact Persons**

**Contact Persons:**

Oriana Badajos, Fishery Biologist I, 907-226-4662, [oriana.badajos@alaska.gov](mailto:oriana.badajos@alaska.gov)

Angela Doroff, Research Coordinator, 907-226-4654, [angela.doroff@alaska.gov](mailto:angela.doroff@alaska.gov)

**Address:**

Kachemak Bay Research Reserve

95 Sterling Highway, Suite 2

Homer, AK 99603

Tel: 907-226-4658

Fax: 907-235-4794

**2) Entry verification**

Deployment data are uploaded from the YSI data logger to a Personal Computer (IBM compatible). Files are exported from EcoWatch in a comma-delimited format (.CDF) and uploaded to the CDMO where they undergo automated primary QAQC; automated depth/level corrections for changes in barometric pressure (cDepth or cLevel parameters); and become part of the CDMO’s online provisional database. All pre- and post-deployment data are removed from the file prior to upload. During primary QAQC, data are flagged if they are missing or out of sensor range. The edited file is then returned to the Reserve for secondary QAQC where it is opened in Microsoft Excel and processed using the CDMO’s NERRQAQC Excel macro. The macro inserts station codes, creates metadata worksheets for flagged data and summary statistics, and graphs the data for review. It allows the user to apply QAQC flags and codes to the data, remove any overlapping deployment data, append files, and export the resulting data file for upload to the CDMO. Upload after secondary QAQC results in ingestion into the database as provisional plus data, recalculation of cDepth or cLevel parameters, and finally tertiary QAQC by the CDMO and assimilation into the CDMO’s authoritative online database. Where deployment overlap occurs between files, the data produced by the newly calibrated sonde is generally accepted as being the most accurate. For more information on QAQC flags and codes, see Sections 11 and 12.

Oriana Badajos was responsible for these tasks.

**3) Research objectives**

The YSI electronic data loggers are programmed to measure the water temperature, specific conductivity, dissolved oxygen, depth, pH, and turbidity conditions at 15-minute intervals. In Kachemak Bay, there are two permanent water quality monitoring stations (Homer and Seldovia), each having two data sondes. One site is located on the northeast side of the Bay at the end of the Homer Spit, and the other on the southwest side of the Bay in Seldovia. At each site, one data logger is suspended 1-meter below the surface (“Surface”), and one data logger is suspended 1-meter from the bottom (“Deep”). At both locations the surface sondes are horizontally within a couple meters of the deep sondes.

The circulation in Kachemak Bay is driven primarily by the 8-meter tidal flux. Regional circulation is characterized by generally cyclonic ocean currents in the Gulf of Alaska flowing onto the shelf off of Cook Inlet. Nutrient rich bottom water is upwelled and mixed with surface water. These enriched waters may enter into Kachemak Bay, the inflow tending to stay along the southern shore flowing past the Seldovia instruments, while water flowing out of the bay stays along the Inner Bay and north shore, flowing past the Homer instruments. These trapped coastal flows separate the bay into two distinct ecosystems, and the instruments are positioned to reflect this distinction. Within each system there is vertical stratification of the water. The vertical placement of the sondes is designed to help elucidate the differences in circulation of the surface and deep waters.

As the inflowing water proceeds up the bay, fresh water runoff from the surrounding ice fields and watersheds dilute the salinity and increase the sediment load in the path of the Homer instruments. The in-flowing water, in the path of the Seldovia instruments, initially supports a marine system, while the northern out-flowing water of the Homer instruments is more estuarine. The Kachemak Bay water quality instruments capture this difference with deployments along the north and south shores. These data will be used to supplement studies on primary productivity, larval distribution, settlement, recruitment, growth rates, community dynamics, and biodiversity in the bay.

**4) Research methods**

Both telemetered instruments (“Deep”) are stationary and housed in ABS pipe mounted vertically on the ferry docks of Homer and Seldovia. The pipes are positioned to ensure that the sensors are approximately 1-meter above the bottom of the ocean floor (actual depth changes with respect to the tides). The surface sondes are attached to a buoy and a sonde guard that slides vertically on a cable to ensure that the sonde remains 1-meter below the surface as the tide is changing.

Calibration and deployment were performed monthly using methods outlined in the YSI Operations Manual. If a rapid pulse DO probe is used, the dissolved oxygen (DO) membrane is replaced and allowed to season in water for at least 6 hours before the DO sensor is calibrated. The following sensors are calibrated using standards purchased from YSI: pH (7 and 10), conductivity (50 mS/cm), and turbidity (123 NTU). Depth is calibrated at zero.

The Chlorophyll probe is calibrated at zero in DI water. QA/QC of this parameter is conducted by comparing sonde data to our monthly grab samples that are analyzed on a Turner 10-AU Spectrophotometer (see Nutrient data/metadata for 2011). Sonde data are accepted or rejected based on this comparison. The estimates of chlorophyll concentration produced by the YSI chlorophyll probe are meant to complement the more accurate results obtained by the monthly grab samples.

A Sutron Sat-Link2 transmitter was installed at the Homer Dolphin Deep station on 12/13/05 and transmits data to the NOAA GOES satellite, NESDIS ID # 3B00077A WQ.

A Sutron Sat-Link2 transmitter was installed at the Seldovia Deep station on 07/31/2007 and transmits data to the NOAA GOES satellite, NESDIS ID # 3B040240 WQ. The transmissions are scheduled hourly and contain four (4) data sets reflecting fifteen minute data sampling intervals. Upon receipt by the CDMO, the data undergoes the same automated primary QAQC process detailed in Section 2 above. The “real-time” telemetry data become part of the provisional dataset until undergoing secondary and tertiary QAQC and assimilation in the CDMO’s authoritative online database. Provisional and authoritative data are available at [http://cdmo.baruch.sc.edu](http://cdmo.baruch.sc.edu/).

**5) Site location and character**

Kachemak Bay is located approximately 200 kilometers south of Anchorage on the western shore of the Kenai Peninsula. Kachemak Bay, at 59.6º N and 151.5º W, is a temperate regional fjord with hydrographic conditions unique among the NERR system estuaries. The tidal range of 8-meters is among the largest in the world, and salinity ranges from near zero at stream mouths to 33.3 PSU at the entrance to the inner Bay. The bay is 35 kilometers wide at its mouth and approximately 57 kilometers long. The head of Kachemak Bay is located to the northeast at the Fox River Flats, and the mouth lies to the southwest, along a line between Anchor Point and Point Pogibshi. The 6-kilometer long Homer Spit that extends into the Bay from the northern shoreline splits Kachemak Bay into inner and outer bays. The Kachemak Bay NERR encompasses both the inner and outer bays. Water flows between the inner and outer Bays through a narrow opening formed between the Spit and the southern shoreline. The Bay has an average depth of 41-meters, and a maximum of 169-meters. Fresh water introduced primarily by the Fox, Bradley, and Martin Rivers and Sheep Creek at the head of the Bay, flows along the northwest shore of the inner Bay.

The Homer YSI data logger site is located on the north side of Kachemak Bay at 59.60203ºN 151.40877ºW. The “deep” sonde is deployed at a depth 1 meter from the bottom, in water fluctuating between 7.5 and 16.8 meters. The “surface” data sonde is deployed at a nominal depth of 1 meter. The bottom habitat is predominantly sand. Pollutants in the area are from the excessive boat traffic at the entrance of the Homer harbor, and a nearby fish waste outfall line. Throughout the year, salinity has ranged from 20.5 to 32.4 ppt, as the instrument's location in the stratified water column is dependent on tide height, with a tidal range of 8.1 meters. It is predominately an estuarine environment during summer months when glacial runoff is highest, and during the winter months it reverts to a more marine-like system with glacial runoff at a minimum.

The Seldovia YSI data logger site is located on the south side of Kachemak Bay at 59.44097ºN 151.72089ºW, approximately 25 kilometers southwest of the Homer site. As with the Homer site, the data loggers are situated on the ferry terminal dock, with one instrument 1 meter below the surface, and one 1 meter above the bottom, in water fluctuating between 4.3 and 13.0 meters. The access to Seldovia is limited to boat or air, as the site is located off the highway system. The bottom habitat is predominantly sand. Pollutants in the area are minimal. Throughout the year, salinity has ranged from 25.0 to 33.9 ppt at this site with a tidal range of 8.0 meters.

**6) Data collection period**

Monitoring at Homer Deep, Seldovia Deep, and Seldovia Surface was continuous throughout 2013. The Homer Surface site was sampled from 03/11/2013 – 12/03/2013, and was removed during the winter months when ice formed on the surface waters at this site. Deployment and retrieval dates and times for 2013 are listed below:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Station** | **Start Date**  **Start Time** | **End Date**  **End Time** | **Sonde ID** | **Comments** |
| Homer Surface 3 | 01/01/2013 00:00 | 03/11/2013 15:15 | None | Not deployed due to ice |
| Homer Surface 3 | 03/11/2013 15:30 | 04/16/2013 14:00 | N |  |
| Homer Surface 3 | 04/16/2013 14:15 | 05/15/2013 08:15 | B |  |
| Homer Surface 3 | 05/15/2013 08:30 | 06/11/2013 12:45 | M |  |
| Homer Surface 3 | 06/11/2013 13:00 | 07/18/2013 10:30 | B |  |
| Homer Surface 3 | 07/18/2013 10:45 | 08/23/2013 12:30 | O |  |
| Homer Surface 3 | 08/23/2013 13:00 | 09/11/2013 12:15 | M | Anchor broke but sonde stayed on cable |
| Homer Surface 3 | 09/13/2013 15:45 | 10/09/2013 10:00 | O | Missed a few days until we purchased a new anchor |
| Homer Surface 3 | 10/09/2013 10:45 | 11/07/2013 11:00 | L |  |
| Homer Surface 3 | 11/07/2013 11:15 | 12/03/2013 13:45 | O | Removed for the winter due to ice |
| Homer Surface 3 | 12/03/2013 14:00 | 12/31/13 23:45 |  | Not deployed due to ice |
|  |  |  |  |  |
| Homer Deep | 12/07/2012 15:30 | 01/08/2013 11:30 | E |  |
| Homer Deep | 01/08/2013 12:00 | 02/04/2013 11:30 | F |  |
| Homer Deep | 02/04/2013 12:15 | 03/11/2013 14:15 | E |  |
| Homer Deep | 03/11/2013 14:45 | 04/04/2013 11:30 | A |  |
| Homer Deep | 04/04/2013 12:00 | 04/16/2013 13:45 | E |  |
| Homer Deep | 04/16/2013 14:00 | 05/15/2013 08:00 | H |  |
| Homer Deep | 05/15/2013 08:30 | 06/12/2013 09:15 | E | Sonde stuck in tube 06/11/2013 12:45 until 06/12/2013 09:15 |
| Homer Deep | 06/12/2013 09:30 | 07/18/2013 10:30 | F |  |
| Homer Deep | 07/18/2013 10:45 | 08/23/2013 12:30 | I |  |
| Homer Deep | 08/23/2013 12:45 | 09/11/2013 12:15 | C |  |
| Homer Deep | 09/11/2013 12:30 | 10/09/2013 09:30 | I |  |
| Homer Deep | 10/09/2013 10:00 | 11/07/2013 11:00 | C |  |
| Homer Deep | 11/07/2013 11:15 | 12/03/2013 13:15 | I |  |
| Homer Deep | 12/03/2013 14:00 | 12/31/13 23:45 | D |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Station** | **Start Date/Time** | **End Date/Time** | **Sonde ID** | **Comments** |
| Seldovia Surface | 12/07/2012 13:15 | 01/09/2013 11:45 | B |  |
| Seldovia Surface | 01/09/2013 12:15 | 02/05/2013 12:30 | M |  |
| Seldovia Surface | 02/05/2013 13:00 | 03/12/2013 14:45 | L | Telemetry platform knocked into water |
| Seldovia Surface | 03/28/2013 13:15 | 04/15/2013 11:15 | M |  |
| Seldovia Surface | 04/15/2013 11:30 | 05/09/2013 12:30 | L |  |
| Seldovia Surface | 05/09/2013 13:00 | 06/03/2013 09:45 | O |  |
| Seldovia Surface | 06/03/2013 10:30 | 07/15/2013 11:45 | C | This sonde was accidently deployed at SS instead of SD (no chl probe) |
| Seldovia Surface | 07/15/2013 12:30 | 08/21/2013 11:15 | M |  |
| Seldovia Surface | 08/21/2013 11:45 | 09/09/2013 12:45 | L |  |
| Seldovia Surface | 09/09/2013 13:30 | 10/11/2013 12:45 | N |  |
| Seldovia Surface | 10/11/2013 13:15 | 11/04/2013 10:15 | M |  |
| Seldovia Surface | 11/04/2013 10:45 | 12/02/2013 11:15 | N |  |
| Seldovia Surface | 12/02/2013 11:45 | 12/31/13 23:45 | M |  |
|  |  |  |  |  |
| Seldovia Deep | 12/07/2012 13:00 | 01/09/2013 11:45 | A | Power surge to sonde; sensor failure |
| Seldovia Deep | 01/09/2013 12:15 | 02/05/2013 12:30 | H |  |
| Seldovia Deep | 02/05/2013 13:00 | 03/12/2013 14:45 | C | Telemetry platform knocked into water |
| Seldovia Deep | 03/28/2013 13:30 | 04/15/2013 11:15 | F |  |
| Seldovia Deep | 04/15/2013 11:30 | 05/09/2013 12:30 | C |  |
| Seldovia Deep | 05/09/2013 13:00 | 06/03/2013 10:15 | F |  |
| Seldovia Deep | 06/03/2013 10:30 | 07/17/2013 10:00 | L | This sonde was accidently deployed at SS instead of SD (has chl) |
| Seldovia Deep | 07/17/2013 10:15 | 08/21/2013 11:15 | C |  |
| Seldovia Deep | 08/21/2013 11:45 | 09/09/2013 12:45 | F |  |
| Seldovia Deep | 09/09/2013 13:15 | 10/11/2013 12:45 | D |  |
| Seldovia Deep | 10/11/2013 13:15 | 11/04/2013 10:30 | F |  |
| Seldovia Deep | 11/04/2013 10:45 | 12/02/2013 11:15 | D | 11/12/13 12:15-12:30; sonde removed from water when troubleshooting |
| Seldovia Deep | 12/02/2013 11:45 | 12/31/13 23:45 | C |  |

**Data collection period (continued)**

**7) Distribution**

NOAA/ERD retains the right to analyze, synthesize and publish summaries of the NERRS System-wide Monitoring Program data. The PI retains the right to be fully credited for having collected and processed the data. Following academic courtesy standards, the PI and NERR site where the data were collected will be contacted and fully acknowledged in any subsequent publications in which any part of the data are used. Manuscripts resulting from this NOAA/OCRM supported research that are produced for publication in open literature, including refereed scientific journals, will acknowledge that the research was conducted under an award from the Estuarine Reserves Division, Office of Ocean and Coastal Resource Management, National Ocean Service, National Oceanic and Atmospheric Administration. The data set enclosed within this package/transmission is only as good as the quality assurance and quality control procedures outlined by the enclosed metadata reporting statement. The user bears all responsibility for its subsequent use/misuse in any further analyses or comparisons. The Federal government does not assume liability to the Recipient or third persons, nor will the Federal government reimburse or indemnify the Recipient for its liability due to any losses resulting in any way from the use of this data.

NERR water quality data and metadata can be obtained from the Research Coordinator at the individual NERR site (please see Principal Investigators and Contact Persons), from the Data Manager at the Centralized Data Management Office (please see personnel directory under the general information link on the CDMO home page) and online at the CDMO home page [http://cdmo.baruch.sc.edu/](http://cfcdmo.baruch.sc.edu/). Data are available in text tab-delimited format.

**8) Associated researchers and projects**

The data are being combined with hydrographic survey data to examine water exchange between Kachemak Bay and Lower Cook Inlet. The sonde data provides the temporal context while the survey data provides the spatial information.

In addition, these data complement the other concurrent System-Wide Monitoring Program modules such as meteorological and nutrient data collection.

**II. Physical Structure Descriptors**

**9) Sensor specifications**

The Kachemak Bay NERR deployed seven 6600EDS sondes and five 6600V4 sondes in 2013. All sondes were deployed with Temperature/Conductivity, pH, turbidity, and ROX DO probes. The V4 sondes were deployed at the surface stations with the same probes as the 6600EDS along with an optical chlorophyll probe.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Parameter** | **Units** | **Sensor Type** | **Model** | **Range** | **Accuracy** | **Resolution** |
| Temperature | Celsius (C) | Thermistor | 6560 | -5 to 50 °C | +/-0.15 °C | 0.01 °C |
| Conductivity | milli-Siemens per cm (mS/cm) | 4-electrode cell with autoranging | 6560 | 0 to 100 mS/cm | +/-0.5% of reading + 0.001 mS/cm | 0.001 mS/cm to 0.1 mS/cm (range dependent) |
| Salinity | parts per thousand (ppt) | Calculated from conductivity and temperature |  | 0 to 70 ppt | +/- 1.0% of reading or 0.1 ppt, whichever is greater | 0.01 ppt |
| Dissolved Oxygen % | percent air saturation (%) | Rapid Pulse – Clark type, polarographic | 6562 | 0 to 500 % air saturation | 0-200 % air saturation, +/- 2 % of the reading or 2 % air saturation, whichever is greater; 200-500 % air saturation, +/- 6 % of the reading | 0.1 % air saturation |
| Dissolved Oxygen mg/L | milligrams per Liter (mg/L); Calculated from % air saturation, temp and salinity | Rapid Pulse – Clark type, polarographic | 6562 | 0 to 50 mg/L | 0 to 20 mg/L, +/- 2 % of the reading or 0.2 mg/L, whichever is greater; 20 to 50 mg/L, +/- 6 % of the reading | 0.01 mg/L |
| Dissolved Oxygen % | % Saturation | Optical probe w/ mechanical cleaning | 6150 ROX | 0 to 500% air saturation | 0-200% air saturation: +/- 1% of the reading or 1% air saturation, whichever is greater; 200-500% air saturation: +/- 15% or reading | 0.1% air saturation |
| Dissolved Oxygen mg/L | milligrams/Liter (mg/L) | Optical probe w/ mechanical cleaning | 6150 ROX | 0 to 50 mg/L | 0-20 mg/L: +/-0.1 mg/l or 1% of the reading, whichever is greater; 20 to 50 mg/L: +/- 15% of the reading | 0.01 mg/L |
| Depth | feet or meters (m) | Stainless steel strain gauge |  | 0 to 30 ft (9.1 m) | +/- 0.06 ft (0.018 m) | 0.001 ft (0.001 m) |
| pH | pH units | Glass combination electrode | 6561 and 6561FG | 0 to 14 units | +/- 0.2 units | 0.01 units |
| Turbidity | nephelometric turbidity units (NTU) | Optical, 90 ° scatter, with mechanical cleaning | 6136 | 0 to 1000 NTU | +/- 2 % reading or 0.3 NTU (whichever is greater) | 0.1 NTU |
| Chlorophyll | micrograms/Liter (μg/L) | Optical probe w/ mechanical cleaning | 6025 | ~0 to 400 μg/L  0 to 100 RFU | The accuracy of the in vivo measurement will be completely dependent on the method of calibration | 0.1 μg/L Chl  0.1% RFU |

**Sensor specifications, continued** (YSI 6600EDS data sonde):

**Dissolved Oxygen Qualifier:**

The reliability of the dissolved oxygen (DO) data after 96 hours post-deployment for non-EDS (Extended Deployment System) data sondes may be problematic due to fouling which forms on the DO probe membrane during some deployments (Wenner et al. 2001). Many reserves have upgraded to the YSI 6600 EDS data sondes, which increases DO accuracy and longevity by reducing the environmental effects of fouling. The user is therefore advised to consult the metadata and to exercise caution when utilizing the DO data beyond the initial 96-hour time period. However, this potential drift is not always problematic for some uses of the data, i.e. periodicity analysis. It should also be noted that the amount of fouling is very site specific and that not all data are affected. The Research Coordinator at the specific NERR site should be contacted concerning the reliability of the DO data because of the site and seasonal variation in the fouling of the DO sensor.

**Depth Qualifier:**

The NERR System-Wide Monitoring Program utilizes YSI data sondes that can be equipped with either vented or non-vented depth/level sensors.  Readings for both vented and non-vented sensors are automatically compensated for water density change due to variations in temperature and salinity; but for all non-vented depth measurements, changes in atmospheric pressure between calibrations appear as changes in water depth.  The error is equal to approximately 1.03 cm for every 1 millibar change in atmospheric pressure, and is eliminated for vented sensors because they are vented to the atmosphere throughout the deployment time interval.

Beginning in 2006, NERR SWMP standard calibration protocol calls for all non-vented depth sensors to read 0 meters at a (local) barometric pressure of 1013.25 mb (760 mm/hg).  To achieve this, each site calibrates their depth sensor with a depth offset number, which is calculated using the actual atmospheric pressure at the time of calibration and the equation provided in the SWMP calibration sheet or digital calibration log.  This offset procedure standardizes each depth calibration for the entire NERR System.  If accurate atmospheric pressure data are available, non-vented sensor depth measurements at any NERR can be corrected.

In 2010, the CDMO began automatically correcting depth/level data for changes in barometric pressure as measured by the Reserve’s associated meteorological station during data ingestion. These corrected depth/level data are reported as cDepth and cLevel, and are assigned QAQC flags and codes based on QAQC protocols. Please see sections 11 and 12 for QAQC flag and code definitions.

**10) Coded variable definitions**

File name definitions: Reserve/deployment site/file definition/year

(ex: kacsswq2013 = Kachemak Bay/Seldovia Surface/WaterQuality/2013).

|  |  |  |
| --- | --- | --- |
| **Sampling station** | **Sampling site code** | **Station code** |
| Homer Surface | HS | kachswq |
| Homer Deep | HD | kachdwq |
| Seldovia Surface | SS | kacsswq |
| Seldovia Deep | SD | kacsdwq |

**11) QAQC flag definitions**

QAQC flags provide documentation of the data and are applied to individual data points by insertion into the parameter’s associated flag column (header preceded by an F\_). During primary automated QAQC (performed by the CDMO), -5, -4, and -2 flags are applied automatically to indicate data that is missing and above or below sensor range. All remaining data are then flagged 0, passing initial QAQC checks. During secondary and tertiary QAQC 1, -3, and 5 flags may be used to note data as suspect, rejected due to QAQC, or corrected.

-5 Outside High Sensor Range

-4 Outside Low Sensor Range

-3 Data Rejected due to QAQC

-2 Missing Data

-1 Optional SWMP Supported Parameter

0 Data Passed Initial QAQC Checks

1 Suspect Data

2 *Open - reserved for later flag*

3 Calculated data: non-vented depth/level sensor correction for changes in barometric pressure

4 Historical Data: Pre-Auto QAQC

5 Corrected Data

**12) QAQC code definitions**

QAQC codes are used in conjunction with QAQC flags to provide further documentation of the data and are also applied by insertion into the associated flag column. There are three (3) different code categories, general, sensor, and comment. General errors document general problems with the deployment or YSI datasonde, sensor errors are sensor specific, and comment codes are used to further document conditions or a problem with the data. Only one general or sensor error and one comment code can be applied to a particular data point, but some comment codes (marked with an \* below) can be applied to the entire record in the F\_Record column.

General Errors

GIC No instrument deployed due to ice

GIM Instrument malfunction

GIT Instrument recording error; recovered telemetry data

GMC No instrument deployed due to maintenance/calibration

GNF Deployment tube clogged / no flow

GOW Out of water event

GPF Power failure / low battery

GQR Data rejected due to QA/QC checks

GSM See metadata

Corrected Depth/Level Data Codes

GCC Calculated with data that were corrected during QA/QC

GCM Calculated value could not be determined due to missing data

GCR Calculated value could not be determined due to rejected data

GCS Calculated value suspect due to questionable data

GCU Calculated value could not be determined due to unavailable data

Sensor Errors

SBO Blocked optic

SCF Conductivity sensor failure

SDF Depth port frozen

SDG Suspect due to sensor diagnostics

SDO DO suspect

SDP DO membrane puncture

SIC Incorrect calibration / contaminated standard

SNV Negative value

SOW Sensor out of water

SPC Post calibration out of range

SQR Data rejected due to QAQC checks

SSD Sensor drift

SSM Sensor malfunction

SSR Sensor removed / not deployed

STF Catastrophic temperature sensor failure

STS Turbidity spike

SWM Wiper malfunction / loss

Comments

CAB\* Algal bloom

CAF Acceptable calibration/accuracy error of sensor

CAP Depth sensor in water, affected by atmospheric pressure

CBF Biofouling

CCU Cause unknown

CDA\* DO hypoxia (<3 mg/L)

CDB\* Disturbed bottom

CDF Data appear to fit conditions

CFK\* Fish kill

CIP \* Surface ice present at sample station

CLT\* Low tide

CMC\* In field maintenance/cleaning

CMD\* Mud in probe guard

CND New deployment begins

CRE\* Significant rain event

CSM\* See metadata

CTS Turbidity spike

CVT\* Possible vandalism/tampering

CWD\* Data collected at wrong depth

CWE\* Significant weather event

**13) Post deployment information**

**Homer Surface (H3):**

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Site** | **Calibration Date** | **Sonde** | **SpCond (50 mS/cm)** | **DO (%)** | **pH (7)** | **pH (10)** | **Turb (0 NTU)** | **Turb (123 NTU)** | **Depth (m)** | **Chl (0)** | **Comments** |
| H3 | 1/3/2013 |  |  |  |  |  |  |  |  |  | Not deployed due to ice |
| H3 | 2/1/2013 |  |  |  |  |  |  |  |  |  | Not deployed due to ice |
| H3 | 3/6/2013 | N | 50.07 | 100.4 | 7.09 | 10.04 | 0.7 | 124.1 | 0.041 | 1.4 |  |
| H3 | 4/12/2013 | B | 49.76 | 98.9 | 6.98 | 10.04 | 1 | 128.3 | -0.089 | 13.8 |  |
| H3 | 5/14/2013 | M | 49.83 | 98.8 | 7.23 | 10.22 | 0.2 | 138.2 | 0.001 | 8.6 |  |
| H3 | 6/7/2013 | B | 49.26 | 104.9 | 7.03 | 10.06 | 0.6 | 119 | 0.058 | 0.1 |  |
| H3 | 7/16/2013 | O | 49.86 | 98.5 | 7.12 | 10.05 | 1.2 | 121.6 | -0.157 | -0.9 |  |
| H3 | 8/23/2013 | M | 49.57 | 99.5 | 7.06 | 10.11 | 0 | 117 | -0.044 | 0.8 |  |
| H3 | 9/6/2013 | O | 50.57 | 96.2 | 7.07 | 10.08 | 1.2 | 120 | -0.108 | 0.2 |  |
| H3 | 10/8/2013 | L | 49.8 | 99.1 | 7.09 | 10.13 | 5.4 | 92.9 | -0.106 | 3.5 |  |
| H3 | 11/1/2013 | O |  |  |  |  |  |  |  |  | Sonde has power issue; will not postcal |
| H3 | 12/3/2013 |  |  |  |  |  |  |  |  |  | Not deployed due to ice |

**Homer Deep (HD):**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Site** | **Calibration Date** | **Sonde** | **SpCond (50 mS/cm)** | **DO (%)** | **pH (7)** | **pH (10)** | **Turb (0 NTU)** | **Turb (123 NTU)** | **Depth (m)** | **Comments** |
| HD | 1/3/2013 | F | 50.34 | 99.1 | 7.12 | 10.11 | 0.3 | 122.8 | -0.155 |  |
| HD | 2/1/2013 | E | 50.07 | 101.3 | 7.02 | 9.85 | 1.1 | 120.8 | 0.039 |  |
| HD | 3/5/2013 | A | 29.54 | 80.2 | 7.14 | 9.73 | 1.5 | 142.6 | -0.042 |  |
| HD | 4/3/2013 | E | 49.92 | 100.2 | 7.03 | 10.11 | 0.7 | 120.3 | 0.047 |  |
| HD | 4/12/2013 | H | 50.96 | 98.9 | 7.04 | 10.04 | 0 | 129.7 | -0.088 |  |
| HD | 5/14/2013 | E | 50.11 | 99.7 | 7.08 | 10.13 | 1.7 | 145.3 | 0.001 |  |
| HD | 6/7/2013 | F | 49.85 | 100.5 | 6.93 | 10.02 | 1.7 | 129.7 | 0.059 |  |
| HD | 7/18/2013 | I | 49.71 | 99.8 | 7.08 | 10.07 | 0.9 | 125.3 | -0.165 |  |
| HD | 8/22/2013 | C | 50.02 | 99.3 | 7.09 | 10.13 | -0.6 | 114.7 | -0.057 |  |
| HD | 9/6/2013 | I | 50.36 | 97.2 | 7.01 | 10.04 | 0.1 | 125.5 | -0.089 |  |
| HD | 10/4/2013 | C | 49.8 | 100.5 | 7.15 | 10.17 | 4.5 | 128 | -0.114 |  |
| HD | 11/1/2013 | I | 51.04 | 103.3 | 7.06 | 10.06 | 0.9 | 125.7 | 0.158 |  |
| HD | 12/3/2013 | D | 50.6 | 100.2 | 6.98 | 10.05 | 1 | 131.1 | 0.051 |  |

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Site** | **Calibration Date** | **Sonde** | **SpCond (50 mS/cm)** | **DO (%)** | **pH (7)** | **pH (10)** | **Turb (0 NTU)** | **Turb (123 NTU)** | **Depth (m)** | **Chl (0)** | **Comments** |
| SS | 1/3/2013 | M | 49.78 | 97.7 | 7.11 | 10.13 | -0.4 | 123.4 | -0.253 | 0 |  |
| SS | 2/1/2013 | L | 50.35 | 99.7 | 7.05 | 10.09 | 0.6 | 120.1 | -0.024 | 0.6 |  |
| SS | 3/5/2013 | M | 50.53 | 100.4 | 7.08 | 10.27 | 0.4 | 127.4 | 0.096 | 1 |  |
| SS | 4/12/2013 | L | 50.79 | 100 | 7.07 | 10.04 | 1 | 113.4 | -0.014 | 0 |  |
| SS | 5/9/2013 | O | 49.47 | 98.1 | 7.07 | 10.14 | 0.6 | 137.6 | -0.081 | 0 |  |
| SS | 5/30/2013 | C | 50.03 | 99.3 | 7.11 | 10.2 | 1.8 | 126.5 | 0.089 |  | Accidently deployed C at SS instead of SD |
| SS | 7/11/2013 | M | 49.93 | 100.3 | 7.06 | 10.12 | 0.9 | 128 | -0.075 | -0.4 |  |
| SS | 8/23/2013 | L | 49.57 | 99.5 | 7.06 | 10.11 | 0 | 117 | -0.044 | 0.8 |  |
| SS | 9/6/2013 | N | 50.84 | 100.9 | 6.97 | 10.01 | -0.1 | 118.5 | -0.04 | -0.2 |  |
| SS | 10/4/2013 | M | 50.07 | 100.2 | 7.01 | 10.05 | -0.1 | 116 | -0.079 | 0.4 |  |
| SS | 11/1/2013 | N | 50.04 | 102.7 | 7.16 | 10.18 | -0.5 | 122.3 | 0.233 | 0.5 |  |
| SS | 11/27/2013 | M | 50.77 | 98.9 | 7.1 | 10.15 | -0.6 | 125.7 | -0.165 | 0 |  |

**Seldovia Surface (SS):**

**Seldovia Deep (SD):**

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Site** | **Calibration Date** | **Sonde** | **SpCond (50 mS/cm)** | **DO (%)** | **pH (7)** | **pH (10)** | **Turb (0 NTU)** | **Turb (123 NTU)** | **Depth (m)** |  | **Comments** |
| SD | 1/3/2013 | H | 50.5 | 98.2 | 7.11 | 10.1 | -1 | 122.2 | -0.255 |  |  |
| SD | 2/1/2013 | C | 49.75 | 100.6 | 7.02 | 10.05 | 1.6 | 120.1 | -0.013 |  |  |
| SD | 3/5/2013 | F | 49.85 | 99.7 | 6.94 | 10.05 | 0.3 | 127.6 | 0.048 |  |  |
| SD | 4/12/2013 | C | 50.3 | 99.8 | 7.1 | 10.06 | 0.2 | 117.9 | 0.007 |  |  |
| SD | 5/9/2013 | F | 49.94 | 100 | 7.08 | 10.07 | 0.3 | 133.5 | -0.071 |  |  |
| SD | 5/30/2013 | L | 49.82 | 101.8 | 7.1 | 10.14 | 0 | 117.2 | 0.078 |  | Accidently deployed L at SD instead of SS |
| SD | 7/16/2013 | C | 49.93 | 100 | 7.23 | 10.31 | 1 | 133.3 | -0.08 |  |  |
| SD | 8/22/2013 | F | 50.02 | 99.3 | 7.09 | 10.13 | -0.6 | 114.7 | -0.057 |  |  |
| SD | 9/6/2013 | D | 51.11 | 101.8 | 7.06 | 10.07 | -0.3 | 121.6 | -0.053 |  |  |
| SD | 10/4/2013 | F | 49.92 | 101 | 6.99 | 10.01 | 0.3 | 122.2 | -0.071 |  |  |
| SD | 11/1/2013 | D | 50.81 | 104.4 | 7.08 | 10.1 | -0.2 | 127.6 | 0.208 |  |  |
| SD | 11/27/2013 | C | 51.33 | 99.3 | 6.98 | 10.05 | 0 | 131.1 | -0.142 |  |  |

**14) Other remarks/notes**

Data are missing due to equipment or associated specific probes not being deployed, equipment failure, time of maintenance or calibration of equipment, or repair/replacement of a sampling station platform. Any NANs in the dataset stand for “not a number” and are the result of low power, disconnected wires, or out of range readings. If additional information on missing data is needed, contact the Research Coordinator at the reserve submitting the data.

Seldovia Surface & Homer Surface sites move up and down on a cable. Sometimes the sonde gets hung-up on the cable, causing out of water events. <1.0 meter and >0.1 meter data are retained.

From 01/01/2013 00:00 - 01/09/2013 11:45 at Seldovia Deep, there was a catastrophic temperature sensor failure due to a power surge. All parameters were rejected during this time period.

On 3/7/13 17:45 the platform that houses our Seldovia deep telemetry gear was thrown into the water. The cause of this is unknown but it may have vandalism. Both sondes were affected and collected data at the wrong depth. All data from 3/7/13 17:45 – 3/12/13 14:45 are rejected. Sondes were removed from the water and not re-deployed until 03/28/13 13:00.

06/11/2013 12:45: Homer Deep sonde was stuck in the PVC tube when trying to remove it. All data were rejected until 06/12/2013 09:15 which is when it was finally unstuck.

From late September- early October 2013, there was a massive bloom of the phytoplankton species *Karenia mikimotoi* covering Kachemak Bay which turned much of the surface water in the bay a dark brown color. This is the first time a large bloom of this species was reported from Alaska, though it is common in many other regions of the world. It is possible that similar blooms have occurred in Alaska the past, but have not been recognized.